**TESTING PROCEDURE**

**TEST SETUP:**

**STEP 2: SET THE MODEL, PLAN AND CHECK ACTUAL QUANTITY**

**Precondition: Connection between PC and the display must be established.**

1. **To change MODEL and PLAN:**

Enter the model name and plan quantity and click on SET button to send the command to the display. If the communication is successful, you will receive a message saying that “Command sent successfully”.

1. **To modify the PLAN:**

Enter plan quantity and click on MODIFY button to send the command to the display. If the communication is successful, you will receive a message saying that “Command sent successfully”.

1. **To modify the ACTUAL:**

Give 24V DC to the input in order to see increment in ACTUAL quantity.